
AudioScience Dante Iyo firmware
###############################

.. contents:: Table of Contents

Known Issues
============


Releases
========

Build v3.5.13 (January 2023)
----------------------------
- lw: fix for inverted GPI

Build v3.5.12 (December 2022)
----------------------------
- hwio: fix for AES67 mode inadvertently persisting 

Build v3.5.11 (May 2022)
----------------------------
- xmos: update XMOS firmware to support A-suffix parts

Build v3.5.9 (January 2022)
----------------------------
- build changes: zip archive upload fix

Build v3.5.8 (January 2022)
----------------------------
- build changes: upload directory path and creates zip of output files

Build v3.5.7 (December 2021)
----------------------------
- wasp: set password to disabled by default

Build v3.5.6 (December 2021)
----------------------------
- same as 3.5.5 but disabled io count test (hanging Travis)

Build v3.5.5 (December 2021)
----------------------------
- same as 3.5.4 but built on master branch

Build v3.5.4 (December 2021)
----------------------------
- note: not built on master branch
- asi27xx: enable ui password with disable

Build v3.5.3 (October 2021)
----------------------------
- oem: add support for OEM serial number
- misc: bugfixes

Build v3.4.2 (September 2021)
-----------------------------
- hwio: reduce unmute delay to 100ms after toggling phantom

Build v3.4.0 (October 2020)
----------------------------
- wasp: update WASP conf files to WASP version 3.2.0
- wasp: support X-Wasp-Stream-Min-Update-Period and X-Wasp-Stream-Exclude-Obj-Type headers

Build v3.3.1 (March 2020)
----------------------------
- dante: fix Dante device prefix names for some models

Build v3.3.0 (March 2020)
----------------------------
- dante: support 88.2kHz sample rate
- audinate: update brooklyn II firmware from 4.0.9.1 to 4.2.0.28
- UI: flash meter LED red when phantom is on; cycle between red and blue when both phantom and mute are on
- UI: always cycle through the complete identify LED identify sequence

Build v3.2.3 (January 2020)
----------------------------
- oem: add support for ASI2791: 4x mic in, 8x line in -> 12x mic/line in

Build v3.2.2 (January 2020)
----------------------------
- py lw: further bug fixes for Pathfinder PC/Pro

Build v3.2.1 (December 2019)
----------------------------
- py lw: fixes for Pathfinder PC/Pro

Build v3.2.0 (November 2019)
----------------------------
- py lw: implement Livewire GPIO

Build v3.1.0 (August 2019)
----------------------------
- webui: add GPIO interface (RJ-45 models)
- webui: modify AES67 interface to allow specific transport IP addresses
- py lw: advertisement bugfix

Build v3.0.0 (July 2019)
----------------------------
- WASP 3.0 (http://www.audioscience.com/internet/download/sdk/wasp/wasp_3.0.0.html)
- support for 14 new DB25 and RJ45 connector models
- AES67 interface UI changes

Build v2.2.2 (June 2019)
----------------------------
- wasp: implement bulk patch support as spcified in version 2.1.0

Build v2.2.1 (May 2019)
----------------------------
- webui: remove non-applicable menu options from Input only and Output models

Build v2.2.0 (March 2019)
----------------------------
- hwio/webui: add output mute
- conf: added OEM configuration

Build v2.1.1 (March 2019)
----------------------------
- hwio: keep SYS led orange until objects restore is complete

Build v2.1.0 (February 2019)
----------------------------
- hwio: cycle input meter LEDs blue when muted
- py: unit test fixes (e.g. property validation)

Build v2.0.1 (January 2019)
----------------------------
- py: HTTP server fixes

Build v2.0.0 (January 2019)
----------------------------
- WASP 2.0: publish specification (http://www.audioscience.com/internet/download/sdk/wasp/wasp_2.0.9.html)
- py: support bulk PATCH methods
- web-ui: improved performance

Build v1.1.0 (December 2018)
----------------------------
- web-ui: add Mute button

Build v1.0.5 (December 2018)
----------------------------
- config: define Product Version

Build v1.0.4 (December 2018)
----------------------------
- hwio/web-ui: add temperature sensor

Build v1.0.3 (November 2018)
----------------------------
- hwio: bug fix for mic pre levels +5 to +10 dBu

Build v1.0.2 (November 2018)
----------------------------
- web-ui: display gain in dB instead of level in dBu on inputs
- http: support method overriding
- hwio/web-ui: bypass pad on input levels of 0 to +10dBu
- web-ui: add Settings tab with LED Brightness option
- models: add ASI2705, ASI2706, ASI2708, ASI2709 (16.0M, 32.0M, 0.16L, 0.32L)
- web-ui: disable phantom power button when pad is engaged
- web-ui: add AES67 streaming feature

Build v1.0.1 (October 2018)
---------------------------

- First release build
